**The emitter transmits a burst of ultrasound to the obstacle positioned in front of the sensor. The object reflects back to sensor receiver the signal and when the echo is received the sensor generates and impulse. LED (light-emitting diode) turns on when the object is detected. To perform this practical click on "Visualize Ckt" button below. Let's get started!!**